,Region##OTHER##,Rated Capacity##HVAC_MASS_PER_TIME##POUNDS_MASS_PER_HOUR,Rated Power##ELECTRICAL_POWER##KILOWATTS,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Rated Current##ELECTRICAL_CURRENT##AMPERES,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Product Documentation Link##OTHER##,Model##OTHER##,Size Models##OTHER##
SKE4-E100-400-3W,E,220.46,74,400,106.5,50,https://www.neptronic.com/Humidifiers/pdf/SKE4/Manuals/2023/SKE4-E-ESA-230914%20(V2.07).pdf,SKE4-E100-400-3W,X
SKE4-E110-400-3W,E,242.51,82,400,118.2,50,https://www.neptronic.com/Humidifiers/pdf/SKE4/Manuals/2023/SKE4-E-ESA-230914%20(V2.07).pdf,SKE4-E110-400-3W,X
SKE4-E120-400-3W,E,264.55,90,400,129.9,50,https://www.neptronic.com/Humidifiers/pdf/SKE4/Manuals/2023/SKE4-E-ESA-230914%20(V2.07).pdf,SKE4-E120-400-3W,X
SKE4-E90-400-3W,E,198.42,66,400,94.8,50,https://www.neptronic.com/Humidifiers/pdf/SKE4/Manuals/2023/SKE4-E-ESA-230914%20(V2.07).pdf,SKE4-E90-400-3W,X
SKE4-E90-440-3W,E,198.42,66,440,86.6,50,https://www.neptronic.com/Humidifiers/pdf/SKE4/Manuals/2023/SKE4-E-ESA-230914%20(V2.07).pdf,SKE4-E90-440-3W,X
SKE4-N100-480-3W,N,100,99.9,480,120.2,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N100-480-3W,X
SKE4-N100-600-3W,N,100,99.9,600,96.1,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N100-600-3W,X
SKE4-N30-2083XW,N,30,29.7,208,82.4,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N30-2083XW,X
SKE4-N40-2083XW,N,40,39.6,208,109.9,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N40-2083XW,X
SKE4-N66-400-3W,N,66,65.7,400,94.8,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N66-400-3W,X
SKE4-N70-480-3W,N,70,69.6,480,83.7,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N70-480-3W,X
SKE4-N70-600-3W,N,70,70,600,72.9,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N70-600-3W,X
SKE4-N74-400-3W,N,74,73.8,400,106.5,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N74-400-3W,X
SKE4-N74-440-3W,N,74,74,440,97.1,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N74-440-3W,X
SKE4-N80-480-3W,N,80,79.8,480,96,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N80-480-3W,X
SKE4-N80-600-3W,N,80,80,600,83.6,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N80-600-3W,X
SKE4-N82-400-3W,N,82,81.9,400,118.2,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N82-400-3W,X
SKE4-N90-400-3W,N,90,90,400,129.9,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N90-400-3W,X
SKE4-N90-440-3W,N,90,90,440,118.1,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N90-440-3W,X
SKE4-N90-480-3W,N,90,90,480,108.3,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N90-480-3W,X
SKE4-N90-600-3W,N,90,90,600,94.3,60,https://www.neptronic.com/Humidifiers/NeptronicDocumentation.aspx,SKE4-N90-600-3W,X

